# Paint Calculator

Estimate the exact amount of paint you need for your interior or exterior walls.

### Project Details

Wall Dimensions (m)
Areas to Exclude (Doors, Windows, etc.)
Number of Doors
Number of Windows
Paint Settings
Coats of Paint

Total Paint Needed

0.00 Liters

/ 0.00 Gallons

Total Wall Area: 0 m²
Excluded Area (Doors/Windows): 0 m²
Total Paintable Area: 0 m²

## The Ultimate Guide to Calculating How Much Paint You Need

Starting a new painting project is exciting, but one of the most common questions that can cause confusion is: "How much paint do I actually need?" Buying too little means a frustrating trip back to the store mid-project, while buying too much is a waste of money. A paint calculator is the perfect solution, providing a precise estimate to ensure you buy the right amount the first time. This guide will explain the factors involved in paint calculation and show you how to use our powerful wall paint calculator for an accurate estimate.

### How to Use Our Advanced Paint Calculator

Our tool is designed to handle simple and complex projects with ease.

1. Select Your Units: At the top of the "Project Details" section, choose between **Metric (m)** for meters or **Imperial (ft)** for feet. All your inputs should be in the selected unit.
2. Enter Wall Dimensions: For each wall you plan to paint, enter its length and height. If you have more than one wall, click the **"+ Add Another Wall"** button to add more input fields.
3. Account for Exclusions: Enter the total number of doors and windows in your project. Our calculator uses standard dimensions to subtract these non-paintable areas, giving you a more accurate result.
4. Specify Coats of Paint: Enter the number of coats you plan to apply. Two coats is standard for most projects for good coverage.
5. View Your Results Instantly: The results on the right will automatically update, showing you:
   - The **Total Paint Needed** in both Liters and Gallons.
   - A detailed breakdown of the **Total Wall Area**, the **Excluded Area** for doors and windows, and the final **Total Paintable Area**.

### The Key Factors in Estimating Paint

A good paint coverage calculator must consider several variables for an accurate result.

#### 1. Total Surface Area

This is the most basic part of the calculation. You need to find the total area of all the surfaces you intend to paint. The formula for the area of a rectangular wall is simple:

`Wall Area = Length × Height`

Our calculator does this for each wall you add and sums them up to get the Total Wall Area.

#### 2. Exclusions (Doors and Windows)

You don't paint over doors and windows, so their area must be subtracted from the total. To simplify the process, our calculator uses standard average dimensions:

- Standard Door Area:** Approximately 1.95 sq. meters (21 sq. feet).
- Standard Window Area:** Approximately 1.4 sq. meters (15 sq. feet).

By subtracting these areas, our room paint calculator ensures you're not buying paint for surfaces that won't be covered.

#### 3. Paint Coverage

This is a crucial factor. "Coverage" refers to how much area a certain amount of paint can cover. The industry standard is:

- 1 Liter of paint** covers approximately **10 square meters** (or 107 square feet).
- 1 Gallon of paint** covers approximately **37 square meters** (or 400 square feet).

Our calculator uses these standard coverage rates. However, keep in mind that this can vary based on the paint brand, the texture of the wall (rough surfaces absorb more paint), and the color you are covering (painting a light color over a dark one may require more paint).

#### 4. Number of Coats

Very rarely is one coat of paint enough for a professional finish. Two coats are standard practice to ensure even color and durability. A primer coat might also be necessary if you are painting on a new, unpainted surface or covering a dark color. Our calculator multiplies the total paintable area by the number of coats you specify to give you the true total amount of paint required.

### Putting It All Together: The Calculation Formula

Our online paint estimator follows this logical sequence:

1. Calculate the total area of all walls.
2. Calculate the total area of all doors and windows to be excluded.
3. Subtract the excluded area from the total wall area to get the `Paintable Area`.
4. Multiply the `Paintable Area` by the `Number of Coats` to get the `Total Coverage Needed`.
5. Divide the `Total Coverage Needed` by the standard coverage per liter/gallon to find the final amount of paint required.

### Frequently Asked Questions (FAQ)

#### Should I buy exactly the amount the calculator suggests?

It's always a good idea to buy a little extra—about 10-15% more. This accounts for any spills, touch-ups, or variations in wall texture. It's better to have a small amount of leftover paint from the same batch than to have to buy a new can later, which might have a slight color variation.

#### Does this calculator work for ceilings?

Yes! To calculate the paint needed for a ceiling, simply treat it as another "wall." Enter the length and width of the ceiling into the length and height fields for a new wall.

#### What if my doors or windows are not standard size?

For the most precise calculation, you can measure the area of your non-standard doors/windows yourself (`Length × Height`). Then, instead of using the door/window input fields, add these as extra "walls" and subtract their total area from your main wall area to find the true paintable surface.

#### How much does 1 litre of paint cover?

As a general rule, 1 litre of standard interior paint will cover about 10 square meters with one coat.

### Conclusion

Proper planning is the key to a successful and stress-free painting project. By using our Paint Calculator, you can eliminate the guesswork and confidently purchase the right amount of paint for your needs. This not only saves you money and time but also ensures you get a professional-looking result without any last-minute hassles. Bookmark this tool for your next DIY project and paint with confidence!